            	                 Tomb Raider
                  Matrox Mystique Accelerated Version 1.03
                              September 4, 1997

This is the update patch to the RETAIL version of Tomb Raider.  This patch
will accelerate Tomb Raider on the Matrox Mystique/Mystique 220 cards. We
didn't think that it was possible, but we now have a Tomb Raider patch for a
2MB Mystique/Mystique 220 card!!  This is the first 2MB Hardware Accelerated
port of the Tomb Raider game!  Note that the Tomb Raider patch works in a
double buffered, hardware Z-buffer, 16bpp color mode.  Hence, in order to
allow such a game with all its amazing worlds and textures to work on a 2MB
card, the game runs in a 512x384 resolution.  Owners of a Mystique/Mystique
220 card of 4MB or 8MB configuration will have an advantage of running at a
resolution of 640x480.  Owners of a Mystique/Mystique 220 card of 4MB or 8MB
configuration who wish to run the game in a 512x384 resolution can set an
environment variable; 'set mtx_lowres=1' before running the game.  Doing a
'set mtx_lowres=0' or 'set mtx_lowres=' will make the game work in 640x480
again.  

If you own a 4MB Mystique/Mystique 220 card with a Rainbow Runner module, you
can see this patch run to TV OUT by setting an environment variable;
'set msi_rr_out=1' before running it.  You must have previously installed the
Rainbow Runner software for Win95.  Also, since the Rainbow Runner module
cannot display a 512x384 resolution out to TV, 2MB Mystique/Mystique 220 users
will not be able to run this Tomb Raider patch out to their TV.


Known problems:

[1] Sometimes, when bringing up the 'Control' option from the Tomb Raider
inventory ring, the game might behave strangely and cause the system to crash.
This does not usually happen in the Title screen but mainly during the game
itself (when pressing Escape to select the 'Control' inventory option).

[2] Certain Joysticks cause the game to behave strangely; such as Lara moving
around in a circle on her own. Please disconnect the Joystick in this case.


Changes since last version:

[1] The last version had problems running on systems with Cyrix CPUs.
[2] This patch now works fine on the Matrox Mystique 220 card.


Installing the MGA Mystique/Mystique 220 patch for Tomb Raider:

1) Install the original game.  If installing under Win95, the game will then
run automatically after the installation is complete.  Please exit the game at
this point as the Mystique patch is not yet enabled.

2) Unzip the tomb_mys.zip file in your Tomb Raider game directory.  The
tomb.exe file should be overwritten and this tomb_mys.txt file will be added.

3) When under Win95, using the AutoRun feature of the Tomb Raider CD-ROM is
the simplest way to run the game.  One could also create a shortcut on the
Win95 desktop.  This shortcut will point to the tomb.pif file which has the
required MS-DOS box properties.  Note that switching to the Win95 desktop
while the game is running will terminate the game.  Even though all the Win95
shortcut keys have been disabled in the tomb.pif, some keyboards still have
the Windows Logo key that will interrupt the game and cause it to be
terminated.  This is a not a great experience if the user didn't get a chance
to save their game!  But, there exists a utility that allows the user to turn
off the Windows Logo key while in a DOS Session.  It is up to the user to find
such a utility.

4) When running under regular DOS, run the game by just typing 'tomb'.
Running the game under regular DOS is recommended for better performance.

A note on savegames: With the Mystique Tomb Raider patch, it is possible to
load savegames that were saved with the VGA version of Tomb Raider.  But, it
is NOT possible to do the opposite (i.e. load Mystique Tomb Raider patch
savegames with the VGA version of Tomb Raider).


Any questions or comments can be directed to Matrox Technical Support at
GRAPH_TS@MATROX.COM

